[Thu Jan  1 08:00:39 1970] [I/sdcard ctl] [sdcard_open]1_N.nc
[Thu Jan  1 08:00:39 1970] [I/sdcard ctl] [sdcard_get_file_stat]get file size 17682460 bytes.
[Thu Jan  1 08:00:39 1970] [I/sdcard ctl] [sdcard_close]1_N.nc 0
[Sat Aug  5 11:49:04 2023] [I/cnc appctl] start nc 1_N.nc from 0 line@Sat Aug  5 03:49:04 2023
[Sat Aug  5 11:49:04 2023] [I/cnc main  ] Enter: cnc_reset
[Sat Aug  5 11:49:04 2023] [I/cnc main  ] Enter: cnc_start_spindle
[Sat Aug  5 11:49:04 2023] [I/cnc spindl] spindle 0 reset
[Sat Aug  5 11:49:04 2023] [I/cnc main  ] Leave: cnc_start_spindle
[Sat Aug  5 11:49:04 2023] [I/cnc main  ] Leave: cnc_reset
[Sat Aug  5 11:49:04 2023] [I/cnc ipt io] dust check on
[Sat Aug  5 11:49:04 2023] [I/cnc out io] dust on.
[Sat Aug  5 11:49:04 2023] [I/cnc main  ] [cnc_start_parser_nc]wrok centor:x@110340,y@146328,z@-96529,a@-207,b@-171,u@0,v@0,w@0 um
[Sat Aug  5 11:49:05 2023] [I/sdcard ctl] [sdcard_open]1_N.nc
[Sat Aug  5 11:49:05 2023] [I/cnc convet] (Head0:HashCode=dd213688004aec3c78d3fcbe5299c908)
[Sat Aug  5 11:49:05 2023] [I/cnc convet] (Head1:NCVer=2)
[Sat Aug  5 11:49:05 2023] [I/cnc convet] (Head2:UPCAMVer=3.0.0.2022.09.15 Date=2022-10-08)
[Sat Aug  5 11:49:05 2023] [I/cnc convet] (Head3:OrderName=2022-10-08-162837 Batch=2 Material=ZIRCONIA Specification=98-16 Machine=P53-DC-X MainModel=2 SubModel=7 JigType=4 BlankId=9 OrderId=40)
[Sat Aug  5 11:49:05 2023] [I/cnc canon ] set g28.2,0x1f
[Sat Aug  5 11:49:05 2023] [I/cnc main  ] Enter: cnc_start_home
[Sat Aug  5 11:49:05 2023] [I/cnc home  ] home axis 2 start
[Sat Aug  5 11:49:05 2023] [I/cnc motion] [MOVE]G90 G53 G1 Z105000 F800 - L105000 - NONE
[Sat Aug  5 11:49:11 2023] [I/cnc canon ] [SMPT]0, 0, 64120, 0, 0, 0, 0, 0, 0, 
[Sat Aug  5 11:49:11 2023] [I/cnc home  ] [HS1 ]64120 um,use 4871 ms
[Sat Aug  5 11:49:11 2023] [I/cnc motion] [MOVE]G90 G53 G1 Z54120 F100 - L10000 - NONE
[Sat Aug  5 11:49:11 2023] [I/cnc canon ] [SMPT]0, 0, 63865, 0, 0, 0, 0, 0, 0, 
[Sat Aug  5 11:49:11 2023] [I/cnc home  ] [HS2 ]255 um,use 202 ms
[Sat Aug  5 11:49:11 2023] [I/cnc motion] [MOVE]G90 G53 G1 Z62865 F100 - L1000 - NONE
[Sat Aug  5 11:49:11 2023] [I/cnc canon ] [SMPT]0, 0, 62865, 0, 0, 0, 0, 0, 0, 
[Sat Aug  5 11:49:11 2023] [I/cnc home  ] [HS3 ]1000 um,use 651 ms
[Sat Aug  5 11:49:11 2023] [I/cnc home  ] home axis 2 finish,NONE

[Sat Aug  5 11:49:11 2023] [I/cnc home  ] home axis 0 start
[Sat Aug  5 11:49:11 2023] [I/cnc motion] [MOVE]G90 G53 G1 X-177000 F800 - L177000 - NONE
[Sat Aug  5 11:49:22 2023] [I/cnc canon ] [SMPT]-135746, 0, 62865, 0, 0, 0, 0, 0, 0, 
[Sat Aug  5 11:49:22 2023] [I/cnc home  ] [HS1 ]135746 um,use 10242 ms
[Sat Aug  5 11:49:22 2023] [I/cnc motion] [MOVE]G90 G53 G1 X-130746 F100 - L5000 - NONE
[Sat Aug  5 11:49:23 2023] [I/cnc canon ] [SMPT]-135461, 0, 62865, 0, 0, 0, 0, 0, 0, 
[Sat Aug  5 11:49:23 2023] [I/cnc home  ] [HS2 ]285 um,use 221 ms
[Sat Aug  5 11:49:23 2023] [I/cnc motion] [MOVE]G90 G53 G1 X-130461 F100 - L5000 - NONE
[Sat Aug  5 11:49:26 2023] [I/cnc canon ] [SMPT]-130461, 0, 62865, 0, 0, 0, 0, 0, 0, 
[Sat Aug  5 11:49:26 2023] [I/cnc home  ] [HS3 ]5000 um,use 3050 ms
[Sat Aug  5 11:49:26 2023] [I/cnc home  ] home axis 0 finish,NONE

[Sat Aug  5 11:49:26 2023] [I/cnc home  ] home axis 1 start
[Sat Aug  5 11:49:26 2023] [I/cnc motion] [MOVE]G90 G53 G1 Y-10000000 F800 - L10000000 - NONE
[Sat Aug  5 11:49:38 2023] [I/cnc canon ] [SMPT]-130461, -158533, 62865, 0, 0, 0, 0, 0, 0, 
[Sat Aug  5 11:49:38 2023] [I/cnc home  ] [HS1 ]158533 um,use 11951 ms
[Sat Aug  5 11:49:38 2023] [I/cnc motion] [MOVE]G90 G53 G1 Y-153533 F100 - L5000 - NONE
[Sat Aug  5 11:49:39 2023] [I/cnc canon ] [SMPT]-130461, -158260, 62865, 0, 0, 0, 0, 0, 0, 
[Sat Aug  5 11:49:39 2023] [I/cnc home  ] [HS2 ]273 um,use 214 ms
[Sat Aug  5 11:49:39 2023] [I/cnc motion] [MOVE]G90 G53 G1 Y-157260 F100 - L1000 - NONE
[Sat Aug  5 11:49:39 2023] [I/cnc canon ] [SMPT]-130461, -157260, 62865, 0, 0, 0, 0, 0, 0, 
[Sat Aug  5 11:49:39 2023] [I/cnc home  ] [HS3 ]1000 um,use 652 ms
[Sat Aug  5 11:49:39 2023] [I/cnc home  ] home axis 1 finish,NONE

[Sat Aug  5 11:49:39 2023] [I/cnc home  ] home axis 3 start
[Sat Aug  5 11:49:39 2023] [I/cnc motion] [MOVE]G90 G53 G1 A-60000 F800 - L60000 - NONE
[Sat Aug  5 11:49:40 2023] [I/cnc canon ] [SMPT]-130461, -157260, 62865, -7453, 0, 0, 0, 0, 0, 
[Sat Aug  5 11:49:40 2023] [I/cnc home  ] [HS1 ]7453 um,use 620 ms
[Sat Aug  5 11:49:40 2023] [I/cnc motion] [MOVE]G90 G53 G1 A352546 F1500 - L360000 - NONE
[Sat Aug  5 11:49:40 2023] [I/cnc canon ] [SMPT]-130461, -157260, 62865, -6753, 0, 0, 0, 0, 0, 
[Sat Aug  5 11:49:40 2023] [I/cnc home  ] [HS2 ]699 um,use 103 ms
[Sat Aug  5 11:49:40 2023] [I/cnc motion] [MOVE]G90 G53 G1 A246 F1500 - L7000 - NONE
[Sat Aug  5 11:49:41 2023] [I/cnc canon ] [SMPT]-130461, -157260, 62865, 246, 0, 0, 0, 0, 0, 
[Sat Aug  5 11:49:41 2023] [I/cnc home  ] [HS3 ]6999 um,use 353 ms
[Sat Aug  5 11:49:41 2023] [I/cnc home  ] home axis 3 finish,NONE

[Sat Aug  5 11:49:41 2023] [I/cnc home  ] home axis 4 start
[Sat Aug  5 11:49:41 2023] [I/cnc home  ] [HS1 ]2400000 um,use 0 ms
[Sat Aug  5 11:49:41 2023] [I/cnc motion] [MOVE]G90 G53 G1 B360000 F1500 - L360000 - NONE
[Sat Aug  5 11:49:48 2023] [I/cnc canon ] [SMPT]-130461, -157260, 62865, 246, 178049, 0, 0, 0, 0, 
[Sat Aug  5 11:49:48 2023] [I/cnc home  ] [HS2 ]178049 um,use 7195 ms
[Sat Aug  5 11:49:48 2023] [I/cnc motion] [MOVE]G90 G53 G1 B180049 F1500 - L2000 - NONE
[Sat Aug  5 11:49:48 2023] [I/cnc canon ] [SMPT]-130461, -157260, 62865, 246, 180049, 0, 0, 0, 0, 
[Sat Aug  5 11:49:48 2023] [I/cnc home  ] [HS3 ]2000 um,use 154 ms
[Sat Aug  5 11:49:48 2023] [I/cnc home  ] home axis 4 finish,NONE

[Sat Aug  5 11:49:48 2023] [I/cnc main  ] Leave: cnc_start_home
[Sat Aug  5 11:49:48 2023] [I/cnc convet] (Roughing cavity side)
[Sat Aug  5 11:49:48 2023] [I/cnc canon ] g0 move short@8 line
[Sat Aug  5 11:49:48 2023] [I/cnc canon ] g0 move short@9 line
[Sat Aug  5 11:49:49 2023] [I/cnc canon ] set m3,spindle speed 0 rpm/min
[Sat Aug  5 11:49:49 2023] [I/cnc canon ] set m7
[Sat Aug  5 11:49:49 2023] [I/cnc canon ] set m6,T1,Q0,mask_0x1
[Sat Aug  5 11:49:49 2023] [I/cnc main  ] Enter: cnc_start_spindle
[Sat Aug  5 11:49:49 2023] [I/cnc spindl] spindle 0 set speed 0 rpm
[Sat Aug  5 11:49:49 2023] [I/rh spindle] spindle set speed for jt driver
[Sat Aug  5 11:49:49 2023] [I/rh spindle] set speed 0 rpm
[Sat Aug  5 11:49:49 2023] [I/rh spindle] use 0 mm
[Sat Aug  5 11:49:49 2023] [I/cnc main  ] Leave: cnc_start_spindle
[Sat Aug  5 11:49:49 2023] [I/cnc main  ] Enter: cnc_start_spindle
[Sat Aug  5 11:49:49 2023] [I/cnc spindl] spindle 0 set mode FLOOD_ON.
[Sat Aug  5 11:49:49 2023] [I/rh spindle] [rh_spindle_set_mode]6.
[Sat Aug  5 11:49:49 2023] [I/cnc main  ] Leave: cnc_start_spindle
[Sat Aug  5 11:49:49 2023] [I/cnc main  ] Enter: cnc_start_change_tool
[Sat Aug  5 11:49:49 2023] [I/cnc tool  ] tool0 change T1,<CRP:x@3345,y@118134>,<CAP:x@-2500,y@-24000> um

[Sat Aug  5 11:49:49 2023] [I/cnc tool  ] [TS1 ]first check cutter
[Sat Aug  5 11:49:49 2023] [I/cnc tool  ] [AT1 ]move z machine zero
[Sat Aug  5 11:49:49 2023] [I/cnc motion] [MOVE]G90 G53 G0 Z0 F0 - L0 - G0_G1_MOVE_DISTANCE_TOO_SHORT
[Sat Aug  5 11:49:49 2023] [I/cnc main  ] [cnc_motion]move too short
[Sat Aug  5 11:49:49 2023] [I/cnc tool  ] [AT2 ]move to CRP
[Sat Aug  5 11:49:49 2023] [I/cnc motion] [MOVE]G90 G53 G0 X3345 Y118134 F0 - L118182 - NONE
[Sat Aug  5 11:49:51 2023] [I/cnc canon ] [SMPT]3345, 118134, 0, 0, 0, 0, 0, 0, 0, 
[Sat Aug  5 11:49:51 2023] [I/cnc tool  ] [AT3 ]move to CAP
[Sat Aug  5 11:49:51 2023] [I/cnc motion] [MOVE]G91 G0 X-2500 Y-24000 F0 - L24129 - NONE
[Sat Aug  5 11:49:52 2023] [I/cnc canon ] [SMPT]845, 94134, 0, 0, 0, 0, 0, 0, 0, 
[Sat Aug  5 11:49:52 2023] [I/cnc tool  ] [AT4 ]start first probe CA
[Sat Aug  5 11:49:52 2023] [I/cnc main  ] Enter: cnc_start_probe
[Sat Aug  5 11:49:52 2023] [I/cnc motion] [MOVE]G90 G53 G1 Z-76835 F800 - L76835 - NONE
[Sat Aug  5 11:49:55 2023] [I/cnc canon ] [SMPT]845, 94134, -39320, 0, 0, 0, 0, 0, 0, 
[Sat Aug  5 11:49:55 2023] [I/cnc probe ] probe success NONE,prb axis 2 -39320um
[Sat Aug  5 11:49:55 2023] [I/cnc main  ] Leave: cnc_start_probe
[Sat Aug  5 11:49:55 2023] [I/cnc tool  ] [AT5 ]move z reverse 3000 um
[Sat Aug  5 11:49:55 2023] [I/cnc motion] [MOVE]G91 G0 Z3000 F0 - L3000 - NONE
[Sat Aug  5 11:49:55 2023] [I/cnc canon ] [SMPT]845, 94134, -36320, 0, 0, 0, 0, 0, 0, 
[Sat Aug  5 11:49:55 2023] [I/cnc tool  ] [AT6 ]start second probe CA
[Sat Aug  5 11:49:55 2023] [I/cnc main  ] Enter: cnc_start_probe
[Sat Aug  5 11:49:55 2023] [I/cnc motion] [MOVE]G91 G1 Z-13000 F80 - L13000 - NONE
[Sat Aug  5 11:49:58 2023] [I/cnc canon ] [SMPT]845, 94134, -39168, 0, 0, 0, 0, 0, 0, 
[Sat Aug  5 11:49:58 2023] [I/cnc probe ] probe success NONE,prb axis 2 -39168um
[Sat Aug  5 11:49:58 2023] [I/cnc main  ] Leave: cnc_start_probe
[Sat Aug  5 11:49:58 2023] [I/cnc tool  ] [AT7 ]move z machine zero
[Sat Aug  5 11:49:58 2023] [I/cnc motion] [MOVE]G90 G53 G0 Z0 F0 - L39168 - NONE
[Sat Aug  5 11:49:59 2023] [I/cnc canon ] [SMPT]845, 94134, 0, 0, 0, 0, 0, 0, 0, 
[Sat Aug  5 11:49:59 2023] [I/cnc tool  ] with cutter,but LST is same

[Sat Aug  5 11:49:59 2023] [I/cnc tool  ] [TS2 ]start put cutter

[Sat Aug  5 11:49:59 2023] [I/cnc tool  ] [TS3 ]check put cutter

[Sat Aug  5 11:49:59 2023] [I/cnc tool  ] [TS4 ]start get cutter

[Sat Aug  5 11:49:59 2023] [I/cnc tool  ] [TS5 ]check get cutter
[Sat Aug  5 11:49:59 2023] [I/cnc tool  ] T1 change finish,NONE,len:32667 um
[Sat Aug  5 11:49:59 2023] [I/cnc canon ] set g43z,32667
[Sat Aug  5 11:49:59 2023] [I/cnc main  ] Leave: cnc_start_change_tool
[Sat Aug  5 11:49:59 2023] [I/cnc canon ] set m3,spindle speed 21000 rpm/min
[Sat Aug  5 11:49:59 2023] [I/cnc canon ] set m8
[Sat Aug  5 11:49:59 2023] [I/cnc convet] (Go to safe)
[Sat Aug  5 11:49:59 2023] [I/cnc canon ] g0 move short@17 line
[Sat Aug  5 11:49:59 2023] [I/cnc canon ] set g43z,32667
[Sat Aug  5 11:49:59 2023] [I/cnc canon ] set g43w,0
[Sat Aug  5 11:49:59 2023] [I/cnc canon ] g1 move short@22 line
[Sat Aug  5 11:49:59 2023] [I/cnc main  ] Enter: cnc_start_spindle
[Sat Aug  5 11:49:59 2023] [I/cnc spindl] spindle 0 set speed 21000 rpm
[Sat Aug  5 11:49:59 2023] [I/rh spindle] spindle set speed for jt driver
[Sat Aug  5 11:49:59 2023] [I/rh spindle] set speed 21000 rpm
[Sat Aug  5 11:50:01 2023] [I/rh spindle] use 2024 mm
[Sat Aug  5 11:50:01 2023] [I/cnc main  ] Leave: cnc_start_spindle
[Sat Aug  5 11:50:01 2023] [I/cnc main  ] Enter: cnc_start_spindle
[Sat Aug  5 11:50:01 2023] [I/cnc spindl] spindle 0 set mode COOLING_ON.
[Sat Aug  5 11:50:01 2023] [I/rh spindle] [rh_spindle_set_mode]4.
[Sat Aug  5 11:50:01 2023] [I/cnc out io] cool 0 on.
[Sat Aug  5 11:50:01 2023] [I/cnc main  ] Leave: cnc_start_spindle
[Sat Aug  5 11:50:04 2023] [I/cnc ipt io] check dust open timeout.
[Sat Aug  5 11:52:38 2023] [I/cnc convet] (Roughing cavity side)
[Sat Aug  5 11:52:38 2023] [I/cnc canon ] set m3,spindle speed 21000 rpm/min
[Sat Aug  5 11:52:38 2023] [I/cnc canon ] set m8
[Sat Aug  5 11:52:38 2023] [I/cnc canon ] g0 move short@24706 line
[Sat Aug  5 11:52:38 2023] [I/cnc canon ] g1 move short@24709 line
[Sat Aug  5 11:52:48 2023] [I/cnc main  ] Enter: cnc_start_spindle
[Sat Aug  5 11:52:48 2023] [I/cnc spindl] spindle 0 set speed 21000 rpm
[Sat Aug  5 11:52:48 2023] [I/rh spindle] spindle set speed for jt driver
[Sat Aug  5 11:52:48 2023] [I/rh spindle] set speed 21000 rpm
[Sat Aug  5 11:52:48 2023] [I/rh spindle] use 0 mm
[Sat Aug  5 11:52:48 2023] [I/cnc main  ] Leave: cnc_start_spindle
[Sat Aug  5 11:52:48 2023] [I/cnc main  ] Enter: cnc_start_spindle
[Sat Aug  5 11:52:48 2023] [I/cnc spindl] spindle 0 set mode COOLING_ON.
[Sat Aug  5 11:52:48 2023] [I/rh spindle] [rh_spindle_set_mode]4.
[Sat Aug  5 11:52:48 2023] [I/cnc out io] cool 0 on.
[Sat Aug  5 11:52:48 2023] [I/cnc main  ] Leave: cnc_start_spindle
[Thu Jan  1 08:00:00 1970] [I/cnc main  ] cnc system initialize start...
[Thu Jan  1 08:00:00 1970] [I/cnc tool  ] tool init successful with 1 cmd table
[Thu Jan  1 08:00:00 1970] [I/cnc spindl] spindle 0 reset
[Thu Jan  1 08:00:00 1970] [I/cnc spindl] spindle 0 init success
[Thu Jan  1 08:00:00 1970] [I/cnc appctl] load parameter table 0 from fram
[Thu Jan  1 08:00:00 1970] [I/cnc canon ] set g92:0, 0, 0, 0, 0, 0, 0, 0, 0, 
[Thu Jan  1 08:00:00 1970] [I/cnc motor ] motor 0 set microstep [256]...0
[Thu Jan  1 08:00:00 1970] [I/cnc motor ] motor 0 set current [1400] mA...0
[Thu Jan  1 08:00:00 1970] [I/cnc motor ] motor 1 set microstep [256]...0
[Thu Jan  1 08:00:00 1970] [I/cnc motor ] motor 1 set current [1400] mA...0
[Thu Jan  1 08:00:00 1970] [I/cnc motor ] motor 2 set microstep [256]...0
[Thu Jan  1 08:00:00 1970] [I/cnc motor ] motor 2 set current [1500] mA...0
[Thu Jan  1 08:00:00 1970] [I/cnc motor ] motor 3 set microstep [256]...0
[Thu Jan  1 08:00:00 1970] [I/cnc motor ] motor 3 set current [1200] mA...0
[Thu Jan  1 08:00:00 1970] [I/cnc motor ] motor 4 set microstep [256]...0
[Thu Jan  1 08:00:00 1970] [I/cnc motor ] motor 4 set current [1200] mA...0
[Thu Jan  1 08:00:00 1970] [I/cnc motor ] motor 5 set microstep [256]...0
[Thu Jan  1 08:00:00 1970] [I/cnc motor ] motor 5 set current [1200] mA...0
[Thu Jan  1 08:00:00 1970] [I/cnc canon ] set g43z,0
[Thu Jan  1 08:00:00 1970] [I/cnc canon ] set g43w,0
[Thu Jan  1 08:00:00 1970] [I/cnc canon ] set g54: 110340, 146328, -96529, -207, -171, 0, 0, 0, 0, 
[Thu Jan  1 08:00:00 1970] [I/cnc tool  ] disable backup tool
[Thu Jan  1 08:00:00 1970] [I/cnc tool  ] set backup tool [T0->T8]
[Thu Jan  1 08:00:00 1970] [I/cnc tool  ] set backup tool [T1->T9]
[Thu Jan  1 08:00:00 1970] [I/cnc tool  ] set backup tool [T2->T10]
[Thu Jan  1 08:00:00 1970] [I/cnc tool  ] set backup tool [T3->T11]
[Thu Jan  1 08:00:00 1970] [I/cnc motor ] motor 0 set sgt [1]...0
[Thu Jan  1 08:00:00 1970] [I/cnc motor ] motor 1 set sgt [3]...0
[Thu Jan  1 08:00:00 1970] [I/cnc motor ] motor 2 set sgt [-2]...0
[Thu Jan  1 08:00:00 1970] [I/cnc motor ] motor 3 set sgt [3]...0
[Thu Jan  1 08:00:00 1970] [I/cnc motor ] motor 4 set sgt [3]...0
[Thu Jan  1 08:00:00 1970] [I/cnc motor ] motor 5 set sgt [4]...0
[Thu Jan  1 08:00:00 1970] [I/cnc tool  ] disable force backup tool,mask(0x0)
[Thu Jan  1 08:00:00 1970] [I/cnc main  ] cnc moudle initialize start...
[Thu Jan  1 08:00:00 1970] [I/cnc main  ] moudle - rgb
[Thu Jan  1 08:00:00 1970] [I/cnc main  ] moudle - ar
[Thu Jan  1 08:00:00 1970] [I/sys boot  ] enter app mode...
[Thu Jan  1 08:00:00 1970] [I/eth server] start listen,fd:0,min:0,max:0
[Thu Jan  1 08:00:00 1970] [I/fpga ctl  ] switch fpga main mode 2
[Thu Jan  1 08:00:00 1970] [I/fpga ctl  ] switch fpga main mode 1
[Thu Jan  1 08:00:00 1970] [I/fpga ctl  ] exit program fpga mode
[Thu Jan  1 08:00:00 1970] [I/fpga ctl  ] fpga find spi device sspi1 successful
[Thu Jan  1 08:00:00 1970] [I/fpga ctl  ] fpga probe flash device sf_fpga successful
[Thu Jan  1 08:00:00 1970] [I/fpga ctl  ] exit program fpga mode
[Thu Jan  1 08:00:00 1970] [I/fpga ctl  ] program done
[Thu Jan  1 08:00:00 1970] [I/fpga ctl  ] exit program fpga mode
[Thu Jan  1 08:00:00 1970] [I/eth server] link up
[Thu Jan  1 08:00:00 1970] [I/fpga ctl  ] check done
[Thu Jan  1 08:00:00 1970] [I/up3d p53  ] fpga init success
[Thu Jan  1 08:00:00 1970] [I/up3d p53  ] file system mnt success
[Thu Jan  1 08:00:04 1970] [I/eth server] dhcp connect fail.set default ip addr.192.168.8.100
[Thu Jan  1 08:02:23 1970] [I/eth server] client(192.168.8.201) connected
[Thu Jan  1 08:02:28 1970] [I/cnc main  ] Enter: cnc_stop
[Thu Jan  1 08:02:28 1970] [I/cnc main  ] Enter: cnc_pasue
[Thu Jan  1 08:02:28 1970] [I/cnc main  ] Enter: cnc_start_spindle
[Thu Jan  1 08:02:28 1970] [I/cnc spindl] spindle 0 stop
[Thu Jan  1 08:02:28 1970] [I/cnc spindl] spindle 0 set mode COOLING_OFF.
[Thu Jan  1 08:02:28 1970] [I/rh spindle] [rh_spindle_set_mode]5.
[Thu Jan  1 08:02:28 1970] [I/cnc out io] cool 0 off.
[Thu Jan  1 08:02:28 1970] [I/cnc spindl] spindle 0 set mode FLOOD_OFF.
[Thu Jan  1 08:02:28 1970] [I/rh spindle] [rh_spindle_set_mode]7.
[Thu Jan  1 08:02:28 1970] [I/cnc spindl] spindle 0 set speed 0 rpm
[Thu Jan  1 08:02:28 1970] [I/rh spindle] spindle set speed for jt driver
[Thu Jan  1 08:02:28 1970] [I/rh spindle] set speed 0 rpm
[Thu Jan  1 08:02:28 1970] [I/rh spindle] use 0 mm
[Thu Jan  1 08:02:28 1970] [I/cnc main  ] Leave: cnc_start_spindle
[Thu Jan  1 08:02:28 1970] [I/cnc canon ] [SMPT]0, 0, 0, 0, 0, 0, 0, 0, 0, 
[Thu Jan  1 08:02:28 1970] [I/cnc main  ] Leave: cnc_pasue
[Thu Jan  1 08:02:28 1970] [I/cnc main  ] Enter: cnc_reset
[Thu Jan  1 08:02:28 1970] [I/cnc main  ] Enter: cnc_start_spindle
[Thu Jan  1 08:02:28 1970] [I/cnc spindl] spindle 0 reset
[Thu Jan  1 08:02:28 1970] [I/cnc main  ] Leave: cnc_start_spindle
[Thu Jan  1 08:02:28 1970] [I/cnc main  ] Leave: cnc_reset
[Thu Jan  1 08:02:28 1970] [I/cnc out io] dust off.
[Thu Jan  1 08:02:28 1970] [I/cnc ipt io] dust check off
[Thu Jan  1 08:02:28 1970] [I/cnc main  ] Leave: cnc_stop
